## Examples of UMT Use Cases

### SNMP-over-IP-over-UMT

Figure 7 presents the example of mapping between SNMP-over-IP to SNMP-over-IP-over-UMT. Individual fields with white background are mapped from the SNMP-over-IP packet to the SNMP-over-IP-over-UMT packet without any changes. Fields with gray background either receive a new value (Destination Address, FCS) or are inserted into the SNMP-over-IP-over-UMT packet (UMT\_Ethertype, UMT\_Subtype\_IPv4, or UMT\_Subtype\_IPv6). Note that the example in Figure 7 applies both to SNMP carried over TCP and SNMP over UDP.



Figure 7: Example of SNMP-over-IP over UMT